****

***Technical Assistance:*** *800-257-5911 or 215-766-2670*

***Email:***[*info@scaletronscales.com*](mailto:info@scaletronscales.com)

***Website:***[*www.scaletronscales.com/downloads*](https://www.scaletronscales.com/downloads/)

**TYPICAL SPECIFICATION FOR MODEL 3000LB™ TON CYLINDER LIFTING BAR**

**Quantity:** A quantity of \_\_\_\_\_\_ Ton Cylinder Lifting Bar(s) shall be provided for securely lifting ton cylinders and containers.

**Construction:** The lifting bar must be constructed from rugged, 2" x 6" x 1/4" steel plate with reinforced pivot points. Heavy-duty hooks must be cut from 1" steel plate and fold inside of body for transport. Bar shall have a lifting bail made of 1" round steel stock and two fork lift carry points. Lifting bar must be protected by a corrosion resistant coating. Coating system shall consist of a zinc oxide primer and dry powder epoxy that is resistant to abrasion, chemicals, moisture and UV light.

**Warranty:** Lifting bar shall carry a full five (5) year factory warranty. “Limited” warranties shall not be accepted.

Lifting bar shall be a Model 3000LB as manufactured by Scaletron Industries Ltd., Plumsteadville, PA.

**Part Number:** 3000LB

**Scaletron™ Industries, Ltd.**  Toll Free: 1-800-257-5911 (USA & Canada)

Bedminster Industrial Park Phone: (+1) 215-766-2670 (International)

53 Apple Tree Lane Fax: (+1) 215-766-2672

P.O. Box 365 E-mail: info@scaletronscales.com

Plumsteadville, PA 18949 USA Website: [www.scaletronscales.com](http://www.scaletronscales.com)

*Page 1 of 1*