****

***Technical Assistance:*** *800-257-5911 or 215-766-2670*

***Email:***[*info@scaletronscales.com*](mailto:info@scaletronscales.com)

***Website:***[*www.scaletronscales.com/downloads*](https://www.scaletronscales.com/downloads/)

**TYPICAL SPECIFICATION FOR MODEL 4042SA™ LEAK DETECTING SPILL ALARM**

**Spill Alarm:** A quantity of \_\_\_\_\_\_ Leak Detecting Spill Alarm(s) shall be provided. The spill alarm must be encased in a corrosion-resistant PVC block. Detector shall have relay contacts rated for 30 VDC and 250 VAC. Detector shall be designed for either 5 VDC or 12 VDC power to match scale indicator in use.

**Cable:** A flexible, four (4) conductor cable with a minimum length of 20 feet shall connect alarm to scale indicator. Cable length shall be \_\_\_\_\_\_ ft. (20 ft. is standard).

**Model/Part Numbers:** 4042SA

Alarm shall be a Model 4042SA as manufactured by Scaletron Industries Ltd., Plumsteadville, PA.

**Scaletron™ Industries, Ltd.**  Toll Free: 1-800-257-5911 (USA & Canada)

Bedminster Industrial Park Phone: (+1) 215-766-2670 (International)

53 Appletree Lane Fax: (+1) 215-766-2672

P.O. Box 365 E-mail: [info@scaletronscales.com](mailto:info@scaletronscales.com)

Plumsteadville, PA 18949 USA Website: [www.scaletronscales.com](http://www.scaletronscales.com/)

*Page 1 of 1*